Technical information 

Wireless access point 

Resetting the access point to original settings 
It may be necessary to reset the access point to a known state in order to add it to the network. 

1. Position the access point so that the front side faces you, with the row of fi\Te LEDs in the lower-right corner. 
2. Disconnect the Ethernet crossover cable and the power adapter. 
3. \X'hile pressing in the switch labeled 51, connect the power adapter to the access point. 
4. Continue pressing 51 until both the Znd and 4th LEDs blink 
simultaneously (approximately 30 seconds). 
5. Release S 1 and wait until the three righ1:most LEDs blink simultaneously (approximately three minutes). -:: 
6. Unplug the power adapter from the power jack on the access point. 

@ 2003 Texas Instruments 

53 

56 

@ 2003 Texas Instruments 

~ccess point LEDs 
Remove the cover to view the LEDs. Position.tlle access point so rhat it faces you, with the LEDs on the right front. 

Battery information for wireless network hubs 
.You cannot damage the batteries by leaving them in the charging bay beyond the time needed to fully charge them. Also. you will not damage the hubs by inserting or removing them from the charging ba)' at any time. 
.It is not necessary to unplug the power adapter from the charging bay. even when no hubs are present. 
.To charge up to four netWork hubs at a time. use the charging bay. It-)'ou only need to charge one netWork hub. you can connect the AC 9930 power adapter directly from the hub to a power outlet. 
.It is not necessaf)' to fully discharge the batteries before recharb.jng them. .To preserve batter}' power, the netWork hub is desib"rled to fall asleep 
after one hour of inactivity. To awaken the hub, remove and then reattach the netWork connector. The hub will also awaken when tlle L.)gIn App is run on any attached handheld or if you reset the hub. Usuall}' a hub dlat has fallen asleep will also awaken if }'OU unplug one of its data cables and then plug it in again. 

Warning: To preserve battery life, remove the network connectors if you need to store the hubs for more than two weeks. 

G> 2003 Texas Instruments 

57